Viewing Configuration

* Install roborun+ program from roboteq
* After installation, while running roborun+, plug USB wire connected directly to motor controller
* A prompt will appear asking to load configuration, click yes

Loading or saving Roboteq configuration

* Go through steps for viewing configuration
* In the first tab, configuration, of robotrun+, on the right there are two buttons for loading profiles or saving profiles from/to disk
* Profiles are in XML form and can be found in Roboteq file in GitHub